marcavettura,"Fiat"
vettura,"Tipo"
tipo,"PS"
telaio,"ZFA35600006517064"
cilindrata,"1600"
potenza,"130"
configurazione,"Pieno + strumentaz. + collaudatore"
altezzaBaricentro,"0.608"
pesoASX,"472.6"
pesoADX,"455.4"
pesoPSX,"287.0"
pesoPDX,"273.6"
panteriore,"62"
passo,"2.635"
carreggiataANT,"1.787"
carreggiataPOST,"1.820"
larghezza,"1.82"
localita,"BALOCCO"
fondostradale,"ALTA_ADERENZA"
richiedente,"Marco Beninati x Andrea Franco"
gruppo,""
commessa,"00"
segmento,""
versione,"CAR"
alimentazione,"Diesel"
posizione,"Trasv. Ant."
trazione,"Anteriore"
cambio,"Manuale"
rapporti,"6"
sterzo,""
marcapneus,"Bridgestone"
tipopneus,"Turanza"
pneuA,"215/55 R17 94V"
pneuP,"215/55 R17 94V"
collaudatore,"Beninati"
progetto,"H2305_23"
data,"24/5/2023"
dataFineProva,"24/8/2023"
SospAnt,""
SospPost,""
BarraAnt,""
BarraPost,""
ContachilometriInizioProva,""
ContachilometriFineProva,""
FasceFrenateProgressive,""
MarcaGDP,""
ModelloGDP,""
DischiAnt,""
PinzeAnt,""
PattiniAnt,""
LottoAnt,""
AntirumoreAnt,""
SmussiAnt,""
DischiPost,""
PinzePost,""
PattiniPost,""
LottoPost,""
AntirumorePost,""
SmussiPost,""
Servo,""
Pompa,""
ABSON,"0"
ABS,""
ABSModel,""
ABSSoftwareVersion,""
EBDON,"0"
Correttore,""
CorsaPedale,""
RapportoPedale,""
AreaPompa,""
DiametroPompa,""
tauprog,"14.70"
tauprogON,"1"
taumed,""
tau30,""
tau30ON,"0"
tau60,""
tau60ON,"0"
tau90,""
tau90ON,"0"
tau120,""
tau120ON,"0"
inerzia,""
pressANT,"2.2"
pressPOST,"2.1"
pesoASX_GVW,""
pesoADX_GVW,""
pesoPSX_GVW,""
pesoPDX_GVW,""
pressANT_GVW,""
pressPOST_GVW,""
pesoASX_LLVW,""
pesoADX_LLVW,""
pesoPSX_LLVW,""
pesoPDX_LLVW,""
tipoCerchioAnt,""
misuraCerchioAnt,""
coppeRuotaAnt,"0"
tipoCerchioPost,""
misuraCerchioPost,""
coppeRuotaPost,"0"
note,"H2305_23: Vettura x prove di addestramento e comparativa lampada ottica"
VDC/ESP,"0"
CDC,"0"
ARC,"0"
Altro,""
acquisitore,"Dewesoft Sirius R2DB s/n D023DC5029"
piattaformaON,"1"
piattX,"0.92"
piattY,"0.73"
piattZ,"0.465"
piattritardo,""
lampadaANTON,"1"
lampANTX,"1.03"
lampANTY,"0.685"
lampANTZ,"0.35"
lampANTritardo,""
lampadaLATON,"0"
lampLATX,""
lampLATY,""
lampLATZ,"0.30"
lampLATritardo,"0.05"
lampadaPOSTON,"0"
lampPOSTX,""
lampPOSTY,""
lampPOSTZ,"0.30"
lampPOSTritardo,"0.05"
satellitareON,"0"
satellitareX,""
satellitareY,""
satellitareZ,""
satellitareritardo,""
altrosensore,""
altrosensoreON,"0"
altrosensoreX,""
altrosensoreY,""
altrosensoreZ,""
altrosensoreritardo,""
laserAntSXCBON,"0"
laserAntSXX,""
laserAntSXY,""
laserAntSXZ,""
laserAntDXCBON,"0"
laserAntDXX,""
laserAntDXY,""
laserAntDXZ,""
laserPostSXCBON,"0"
laserPostSXX,""
laserPostSXY,""
laserPostSXZ,""
laserPostDXCBON,"0"
laserPostDXX,""
laserPostDXY,""
laserPostDXZ,""
TipoGPS,""
GPS_X,""
GPS_Y,""
GPS_Z,""
GPS_Vel,""
GPS_Dir,""
GPS_Dist,""
GPS_Sat,""
GPS_Acc,""
canalicalc,""
strumanalogica,"A1;DVOL;Angolo volante;RMS;17437;DVOL_50;50;Deg/V;;0.003;13-7-2023;
A2;COPPIAV;Coppia volante;RMS;17437;COPPIAV_10;10;Nm/V;;0.011;13-7-2023;
A3;BETA;Angolo assetto;Kistler;4837260;Beta;-4;°/V;;0.065;9-12-2024;
A4;VEL;Velocità veicolo;Kistler;4837260;Vel;40;Kph/V;;0.065;9-12-2024;
A5;AY;Acc laterale;Gladiator;258;AY;0.4;g/V;5V;0.007;28-10-2024;
A6;PSIP;Vel imbardata;Gladiator;258;Psip;30;Deg/sec/V;5V;0.007;28-10-2024;
A7;THETAP;Vel rollio;Gladiator;258;Thetap;30;Deg/sec/V;5V;0.007;28-10-2024;
A8;AX;Acc longitudinale;Gladiator;258;AX;0.4;g/V;5V;0.007;28-10-2024;
B1;PHIP;Vel beccheggio;Gladiator;258;Phip;30;Deg/sec/V;5V;0.007;28-10-2024;
"
strumdigitale,""
strumcounter,""
CAN0,""
CAN1,""
prove,""
piste,""
